Data available at materials.hybrid3.duke.edu/materials/dataset/1481

Reference: B. Febriansyah, T. Koh, Y. Lekina, N. Jamaludin, A. Bruno, R. Ganguly, Z. Shen, S. Mhaisalkar, J. England, "Improved Photovoltaic Efficiency and Amplified Photocurrent Generation in Mesoporous n = 1 Two-Dimensional Lead−Iodide Perovskite Solar Cells", Chemistry of Materials 31, 890  (2019)

Origin: experimental
Sample type: single crystal

Physical property: atomic structure, Å

Fixed parameters:
  temperature = 100.0 K
a 6.3354 (±0.0003) Å
b 19.8007 (±0.0009) Å
c 12.5707 (±0.0005) Å
α 90°
β 90.757 (±0.002)°
γ 90°


