Data available at materials.hybrid3.duke.edu/materials/dataset/1487

Reference: B. Febriansyah, T. Koh, Y. Lekina, N. Jamaludin, A. Bruno, R. Ganguly, Z. Shen, S. Mhaisalkar, J. England, "Improved Photovoltaic Efficiency and Amplified Photocurrent Generation in Mesoporous n = 1 Two-Dimensional Lead−Iodide Perovskite Solar Cells", Chemistry of Materials 31, 890  (2019)

Origin: experimental
Sample type: single crystal

Physical property: atomic structure, Å

Fixed parameters:
  temperature = 100.0 K
a 12.4948 (±0.0003) Å
b 19.7152 (±0.0004) Å
c 12.5841 (±0.0003) Å
α 90°
β 96.4396 (±0.0008)°
γ 90°


