Data available at materials.hybrid3.duke.edu/materials/dataset/1864

Reference: A. Singh, M. Jana, D. Mitzi, "Reversible Crystal–Glass Transition in a Metal Halide Perovskite", Advanced Materials 33, 2005868  (2020)

Origin: experimental
Sample type: single crystal

Physical property: atomic structure

Fixed parameters:
  Melting Point = 175.0 °C
  Glass transition temperature = 67.0 °C
  Degradation onset temperature = 204.0 °C
  Crystallization onset temperature (Beginning from glass) = 101.0 °C
a 8.7537 (±0.00019) 
b 7.95502 (±0.00016) 
c 19.5038 (±0.0005) 
α 90°
β 93.806 (±0.002)°
γ 90°


